|  |  |
| --- | --- |
| **U.S. Radiocommunications Sector**  **Fact Sheet** | |
| **Working Party:** USWP7C | **Document No:** US 7C/27-027NC |
| **Reference:**  R23-WP7C-C-0041!N02 | **Date:** 12 August 2024 |
| Document Title: Preliminary draft revision of Report ITU-R RS.2489-0 | |
| **Author(s)/Contributors(s):**  Philip Sohn  DOC/NOAA/NWS  Tomasz Wojtaszek  DOC/NOAA  Christopher Hough  DOC/NOAA  Edna Prado  DOC/NOAA | Phone: 301-427-9676  Email: [philip.sohn@noaa.gov](mailto:philip.sohn@noaa.gov)  Phone : 301-456-4574  Email : [tomasz.wojtaszek@noaa.gov](mailto:tomasz.wojtaszek@noaa.gov)  Phone : 301-323-8212  Email : [christopher.hough@noaa.gov](mailto:christopher.hough@noaa.gov)  Phone : 301-628-5742  Email : [edna.prado@noaa.gov](mailto:edna.prado@noaa.gov) |
| Purpose/Objective: To propose updates to the preliminary draft revision of Report ITU-R RS.2489-0 regarding technical and operational characteristics of ground-based passive sensors operating in the 22-32 GHz and 51-58 GHz frequency ranges. | |
| **Abstract:**  This contribution seeks to provide editorial updates and additional material to the preliminary draft revision of Report ITU-R RS.2489-0 in support of further progressing the work on documenting technical and operational characteristics of ground-based passive radiometers operating in the 22-32 GHz and 51-58 GHz frequency ranges in support of meteorological applications and research. | |
| **Fact Sheet Preparer:** Philip Sohn | |

|  |  |
| --- | --- |
| **Radiocommunication Study Groups** |  |
|  |  |
|  |  |
| Source: R23-WP7C-C-0041!N02  Subject: PDRR ITU-R RS.2489-0 | **Document 7C/** |
| **XX September 2024** |
| **English only** |
| United States of America | |
| PRELIMINARY DRAFT REVISION OF REPORT ITU-R RS.2489-0 | |
| Technical and operational characteristics of ground-based passive sensors operating in the 51-58 GHz frequency range | |

**Introduction**

This contribution provides editorial updates and additional material to the preliminary draft revision of Report ITU-R RS.2489-0 that was attached as Annex 2 to the report on the meeting of working party 7C (18-22 March 2024).

**Attachment**: 1

ATTACHMENT

PRELIMINARY DRAFT REVISion OF REPORT ITU-R RS.2489-0

Technical and operational characteristics of ground-based passive sensors operating in the 22-32 GHz and 51-58 GHz frequency ranges

(2021-202X)

Summary of revision

This revision provides updates of ground based passive sensor systems using radio spectrum which are used for observations of the temperature and the water vapor profile of the atmosphere.

Keyword

Ground-based passive radiometers, meteorology, climatology

# 1 Introduction

This Report provides technical and operational characteristics of ground-based passive microwave radiometers in the 22-32 GHz and 51-58 GHz ranges, used for observations of the temperature of the atmosphere. The use of these radiometers supports meteorological applications and research by providing measurements of the profile of temperature in the lowest several kilometers of the atmosphere, integrated water vapor, and integrated cloud liquid water. Ground-based radiometers could be used for local atmosphere observations or in the framework of worldwide observational networks.

Microwave radiometers are very sensitive receivers designed to measure thermal electromagnetic radiation emitted by atmospheric gases. They are usually equipped with multiple receiving channels in order to derive the characteristic emission spectrum of the atmosphere.

It has to be noted that in some cases these ground based sensors are operating opportunistically and outside frequency bands allocated to passive operations and without any protection.

# 2 Meteorology/climatology usages

Microwave radiometers are utilized in a variety of environmental and engineering applications, including weather forecasting and nowcasting, climate monitoring, radio propagation studies and radio astronomy.

Worldwide vertical profiles of atmospheric temperature are provided by several types of satellites (polar-orbiting satellites equipped with microwave sounding instruments) but meteorologists making detailed local forecasts or scientists investigating the planetary boundary layer[[1]](#footnote-1) have requirements for atmospheric sounding with better vertical resolution than can be provided by the satellite radiometers. This higher resolution information can be provided by using an upward-looking passive remote sensor, with a radiometer mounted at the Earth’s surface. Also, the coincident measurements of integrated water vapor and cloud liquid water are critical observations to a range of research and operational applications.

Passive microwave radiometry is a tool of fundamental importance for the Earth observation and radiometers are designed to receive and measure natural emissions produced by the Earth’s surface and its atmosphere. Ground-based radiometers are well suited to measure temperature profiles in the lower part of the atmosphere: the troposphere.

Microwave sensors can provide an almost all-weather capability due to higher transmission through clouds at microwave than at visible or infrared wavelengths; only at moderate to high rain rates are the observations from ground-based microwave radiometers negatively impacted. This near all-weather capability has considerable interest for the Earth observation because more than 60% of the Earth’s surface is usually covered with clouds. In addition to this capability, passive microwave measurements can also be taken at any time of day as they are not reliant on daylight. Passive microwave sensing is an important tool widely used for meteorological, climatological, and environmental monitoring and survey (operational and scientific applications), for which reliable repetitive global coverage is essential.

Commercial ground radiometers from multiple vendors are now available for meteorological operational applications.

## 2.1 Frequency aspects

A selection of channels between:

– 22 GHz and 28 GHz are used to provide information on the variation of water vapour in the vertical profile, a window observation in the region of 30 GHz is also used for integrated cloud liquid water observations

– 50 GHz and 58 GHz are used to produce a measurement of temperature structure.

Figure 1 shows the down-welling thermal emission of the atmosphere expressed in term of brightness temperature, as seen by a sensor deployed at sea level (blue) and at 4.5 km altitude (red). The oxygen emission lines that form the absorption complex around 60 GHz, some of which are visible in the red curve, together with the positions and bandwidths of the channels of an idealized radiometer. Given the increasing opacity of the atmosphere going toward the centre of the absorption complex at 60 GHz, the radiation reaching the sensor in different channels is emitted by shallower atmospheric layers. The channel at 58 GHz receives radiation from an approximately 500 m-thick layer while the channel at 52 GHz has contributions from the whole troposphere, hence the different brightness temperatures. A proper retrieval algorithm can then reconstruct the atmospheric temperature profile using the measurements of the various channels.

Figure 1

Simulated spectrum for ground-based radiometer between 50 and 60 GHz

Chart, histogram

Description automatically generated

*Note to Fig. 1*: The blue line is used for a sensor at sea level, and the red line for a sensor at 4.5 km of altitude. The channels measured by the instruments are marked in grey.

Figure 2 shows the sensitivity of millimeter and sub-millimeter frequencies to atmospheric temperature and water vapour variations between 1 and 275 GHz. The water vapour and oxygen resonance spectral lines are indicated in the figure as well.

Figure 2

Atmospheric opacity in frequency range 1-275 GHz



Although the channels for ground based remote sensing of temperature are in the same spectral region to passive satellite remote sensing, they are not identical frequencies to those used by satellites. At some frequencies, satellite remote sensing can safely share with terrestrial services, but ground‑based radiometers may need protection in order to be effective. The number of ground‑based radiometers in operation is still small, but if current developments are successful, larger numbers may be deployed in the future.

## 2.2 Typical characteristics

Table 1 below shows some typical characteristics of commercial ground-based passive radiometers deployed in the frequency range 22-31 GHz and 51‑58 GHz. Scientific radiometers could have less system temperature in case of cooled receiving system.

The sensitivity of these radiometers is done by the radiometric equation and dependent on the system temperature, the integration time and the integrated bandwidth. The typical operational integration time for measurements is two seconds. For calibration of the radiometer, the integration time has to be defined. To specify the interference threshold level, the error rate compared to sensitivity has also to be defined.

TABLE 1

Typical characteristics of commercial ground-based passive radiometers

|  |  |  |
| --- | --- | --- |
| Platform type (airborne, ship borne, ground) | Ground | Ground |
| Channel center frequencies | 22.24 GHz, 23.04 GHz, 23.84 GHz, 25.44 GHz, 26.24 GHz, 27.84 GHz, 31.4 GHz | 51.26 GHz, 52.28 GHz, 53.86 GHz, 54.94 GHz, 56.66 GHz, 57.3 GHz, 58.0 GHz |
| Antenna type (reflector, phased array, slotted array, etc.) | Corrugated feedhorn + reflector | Corrugated feedhorn + reflector |
| Antenna diagram | Gaussian beam | Gaussian beam |
| Antenna sidelobe level (dB) | < −30 | < −30 |
| Antenna main beam gain (dBi) | 33 | 40 |
| Antenna height (m) | 1.2 | 1.2 |
| Receiver noise figure (dB) | 2 | 2.5 |
| System noise temperature (°K) | 400 | 600 |
| Receiver RF 3 dB bandwidth (MHz) | 230 | 600-2 000 |
| Geographical distribution | Worldwide | Worldwide |
| Fraction of time in use (%) | 100 | 100 |
| Integration time (s) | 2 | 2 |

## 2.3 Worldwide deployments for meteorological radiometers

Currently, it is estimated that more than 200 ground-based passive radiometers are deployed in the frequency range 22-31 GHz and 51‑58 GHz on a worldwide basis.

Figure 3 shows the location of these systems.

FIGURE 3

Location of ground-based passive radiometers in the 22-31 GHz and 51-58 GHz

A map of the world with orange pointers

Description automatically generated

### 2.3.1 ITU Region 1

In Switzerland, ground-based passive sensors, and specifically microwave radiometers, are an important component of the [EMER-Met](https://www.meteoswiss.admin.ch/weather/warning-and-forecasting-systems/meteorology-for-nuclear-accidents.html) (Emergency-Response Meteorology) system. This system monitors the atmosphere with wind profiler radars and microwave radiometers to measure the temperature and humidity profiles from the ground up to an altitude of several kilometers. These local observation data are integrated in real time into a high-resolution numerical weather prediction model for the provision of emergency management in the case of nuclear accidents in Switzerland and neighboring countries.

Three sites are currently in operation: Payerne in the southwest, Schaffhausen in the north-east and Grenchen in the centre of the Swiss Plateau. The [EMER-Met](https://www.meteoswiss.admin.ch/weather/warning-and-forecasting-systems/meteorology-for-nuclear-accidents.html) system has been operational since 2010 and it shows an availability rate of over 95%. This system, that relies on microwave radiometers, is essential in Switzerland for strategic decision-making in the event of a nuclear accident.

### 2.3.2 ITU Region 2

In the United States, a 2009 National Research Council recommendation included deployment of ground-based microwave radiometers at approximately 400 sites as a high infrastructure priority to continually monitor lower tropospheric conditions and fill many of the critical gaps in the national observing system.  Currently, the New York State Mesonet (NYSM) Profiler Network is operating seventeen profiler sites across the state as a national testbed to facilitate research and evaluation of ground-based passive sensors and their applications.  Additionally, it is estimated that there are fifty or more microwave radiometers in use by various organizations to support meteorological applications and research in the United States.

# 3 Summary

There is an interest in ground-based passive radiometers in the 22-31 GHz and 51-58 GHz ranges, used by meteorological, climate change, satellite communication and astronomy communities. This Report presents the usage of such systems in particular regarding the need to obtain better vertical resolution for atmospheric temperature profile near the ground in order to provide more detailed local forecasts.

Characteristics of commercial ground-based passive radiometers for meteorological application operating in the frequency ranges 22-31 GHz and 51‑58 GHz have been developed.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. In meteorology, the planetary boundary layer (PBL), also known as the atmospheric boundary layer (ABL), is the lowest part of the atmosphere. Its behaviour is directly influenced by its contact with a planetary surface. [↑](#footnote-ref-1)